Build and execute by running Python laptop1.py.

Enter 1 for Console Key entry or 2 for File transfer.

Laptop 1 will send packets to raspberry PI via socket and wait for ACK response from raspberry PI.